##

07.2 Carburetor - M115

- 07.2-090 - Layout and operation of Stromberg carburetor standard version
- 07.2-096 - C. (USA) model year 1974-1976
- 07.2-100 - Adjusting idle speed
- 07.2-102 - Checking idle speed shutoff valve
- 07.2-104 - Removal and installation of idle speed shutoff valve
- 07.2-105 - Checking, correcting basic adjustment of throttle valve
- 07.2-107 - Checking, correcting basic adjustment of fuel adjusting screw (national version only)
- 07.2-110 - Checking, regulating engine
- 07.2-125 - Checking, adjusting choke
- 07.2-128 - Performing cold start
- 07.2-136 - Replacing diaphragm for choke
- 07.2-137 - Replacing drive lever in choke
- 07.2-140 - Removing, checking and installing choke
- 07.2-142 - Checking, correcting choke housing mark
- 07.2-149 - Subsequent installation of standard choke housing

> Carburetor (general)

- 07.2-180 - Checking, adjusting float valve
- 07.2-182 - Checking float chamber venting system (national version only)
- 07.2-186 - Checking fuel return valve
- 07.2-190 - Cleaning, adjusting carburetor
- 07.2-194 - Removal and installation of carburetor
- 07.2-195 - Removal and installation of air piston, air piston diaphragm and nozzle needle

> Fuel pump

- 07.2-210 - Testing fuel pump
- 07.2-212 - Removal and installation of fuel pump

###

Copyright © 2003, 2004 Steve Nervig.
All Rights Reserved