##

33 Front Axle

- Bad Wheel Bearing?

> Front axle halves

- 33-200 - Removal and installation of front axle half

> Front wheel hub

- 33-300 - Adjustment of wheel bearing and play
- 33-310 - Removal and installation of front wheel hub
- 33-320 - Disassembly, inspection, repair and assembly of front wheel hub

> Steering knuckle

- 33-400 - Removal and installation of steering knuckle
- 33-410 - Checking the steering knuckle
- 33-420 - Removal and installation of steering knuckle arm

> Steering knuckle bearing

- 33-425 - Checking supporting and guide joint of steering knuckle bearing
- 33-430 - Replacement of sleeves for supporting and guide joint of steering knuckle bearings
- 33-440 - Replacement of supporting joint for steering knuckle bearing

> Control arm

- 33-500 - Removal and installation of upper control arm
- 33-512 - Removal, disassembly, assembly and installation of lower control arm
- 33-515 - Removal and installation of brake support
- 33-520 - Reconditioning bearing of lower control arm
- 33-540 - Checking supporting joint and supporting tube of brake support
- 33-550 - Checking and reconditioning bearing of upper control arm
- 33-560 - Checking upper control arm
- 33-570 - Checking lower control arm

###

Copyright © 2003, 2004 Steve Nervig.
All Rights Reserved