##

54 Chassis Electrical, Instruments

> Battery and grounding points

- Battery Cradle Inspection and Cleanup
- 54-005 - Battery test, service and maintenance
- 54-100 - Designation and layout of grounding points

> Instruments

- 54-250 - Removal and installation of instrument cluster
- 54-251 - Removal and installation of indicating instruments
- 54-253 - Removal and installation of tachometer
- 54-256 - Function immersion tube transmitter for fuel gauge
- 54-257 - Testing fuel gauge
- 54-258 - Removal and installation of time clock
- 54-270 - Pressure difference warning system wiring diagram [USA] 1977

> Switch, switch console, wiring diagrams - special versions, ash tray, etc

- 54-305 - Removal and installation of rotary light switch
- 54-310 - Removal and installation of combination switch
- 54-312 - Testing, refinishing resetting of turnsignal arm
- 54-320 - Removal and installation of rear dome lamp and switch, T-sedan
- 54-325 - Removal and installation of turnsignal lamp and warning flasher switch with relay
- 54-326 - Layout warning flasher relay starting September 1981
- 54-340 - Removal and installation of switch console
- 54-350 - Wiring diagram special versions for fog lamp, headlamp flasher, backup lamp
- 54-390 - Renewing bulbs of control system, heater
- 54-391 - Renewing bulb for ashtray light
- 54-410 - Seatbelt warning device, ignition key, lamps [USA] starting 1978

> Cruise control, pneumatic

- 54-500 - Cruise control operation
- 54-505 - Checking the actuator
- 54-510 - Checking switch, control unit and line harness
- 54-515 - Checking switch
- 54-520 - Checking sensor
- 54-525 - Checking cable control
- 54-530 - Checking control unit
- 54-540 - Removal and installation of actuator
- 54-545 - Removal and installation of switch
- 54-550 - Removal and installation of sensor on mechanical tachometer
- 54-555 - Removal and installation of cable control
- 54-560 - Adjustment of cable control
- 54-565 - Removal and installation of control unit
- 54-570 - Vacuum connection for throttle servo unit
- 54-575 - Removal and installation of switch on clutch pedal
- 54-580 - Wiring diagram

> Cruise control / Tempomat, electric

- 54-500a - Cruise control operation
- 54-504a - Testing with adapter
- 54-506a - Testing coding plug
- 54-541a - Removal and installation of actuator
- 54-545a - Removal and installation of switch
- 54-550a - Removal and installation of sensor on mechanical tachometer
- 54-561a - Adjustment of connecting rod
- 54-565a - Removal and installation of control unit
- 54-575a - Removal and installation of switch on clutch pedal
- 54-577a - Removal and installation of relay decel shutoff / cruise control

###

Copyright © 2003, 2004 Steve Nervig.
All Rights Reserved