##

91 Seats and Restraints

> Front seat

- 91-100 - Removal and installation of front seat (driver's seat)
- 91-110 - Removal and installation of front seat (passenger's seat)
- 91-112 - Construction and operation of the seat back locking system
- 91-115 - Remove and install vacuum element from driver's or co-driver's seat (coupe)
- 91-117 - Remove and install door contact vacuum switch (coupe)
- 91-119 - Remove and install vacuum switch of driver's seat back (coupe)
- 91-120 - Removal and installation of reclining seat fittings
- 91-150 - Check seat back locking system (coupe)
- 91-162 - Function schematic seat back locking system (coupe)
- 91-165 - Removal and installation, reconditioning of folding armrest for driver's seat

> Rear seat

- 91-170 - Removal and installation of rear seat and rear seat backrest

> Electrostatic discharge

- 91-300 - Remedy for electrostatic discharge on seats

> Safety belts

- 91-500 - Removal and installation of safety belt
- 91-550 - Exchange instructions for safety belt

###

Copyright © 2003, 2004 Steve Nervig.
All Rights Reserved