##

32 Suspension, Level Control System

- George Murphy on installing shocks

> Springs - shock absorbers

- 32-010 - Permissible combinations springs - shock absorbers

> Shock absorbers

- 32-100 - Removal and installation of front shock absorber
- 32-110 - Removal and installation of rear shock absorber
- 32-120 - Checking shock absorber
- 32-125 - Checking alignment of front shock absorbers
- 32-126 - Checking alignment of rear shock absorbers

> Springs

- 32-200 - Removal and installation of front spring
- 32-205 - Removal and installation of front spring (in combination with R&I of front axle half after an accident)
- 32-220 - Adjustment of front springs
- 32-230 - Removal and installation of rear springs
- 32-240 - Adjustment of rear springs
- 32-250 - Test value of springs

> Torsion bars

- 32-300 - Removal and installation of torsion bar on front axle
- 32-310 - Removal and installation of torsion bar on rear axle

> Level control system and inspections

- 32-501 - Functional description
- 32-510 - Checking spring struts
- 32-520 - Checking pressure reservoir
- 32-530 - Checking pressure oil pump and level controller

> Assembly jobs

- 32-610 - Removal and installation of spring struts
- 32-612 - Checking and replacing suspension of spring strut (T-sedans)
- 32-620 - Removal and installation of pressure reservoir
- 32-630 - Draining and filling of pressure oil system
- 32-640 - Removal and installation of pressure oil pump
- 32-641 - Conversion of suction and pressure line on model 123 with diesel engine 3rd version
- 32-645 - Replacement of radial sealing ring for pressure oil pump
- 32-660 - Removal and installation of connecting rod of level controller
- 32-670 - Removal and installation of level controller
- 32-671 - Conversion of oil lines between level controller and pressure reservoir in the event of complaints about noise

###

Copyright © 2003, 2004 Steve Nervig.
All Rights Reserved