##

07.1 Diesel Injection System - OM617

> Testing and adjusting jobs

- 07-001 - Survey engine model injection pump
- 07-010 - Operation of injection pump and rpm governor
- 07-100 - Adjustment of idle speed and idle speed adjuster
- 07-105 - Inspection and adjustment of no-load max speed
- 07-109 - Checking injection pump for begin of delivery (according to high pressureoverflow method)
- 07-110 - Checking injection pump for begin of delivery (according to low pressure-overflow method)
- 07-115 - Adjusting injection pump for begin of delivery (after checking begin of delivery)
- 07-120 - Checking injection pump for offset of begin of delivery (after checking begin of delivery of cylinder 1)
- 07-125 - Checking pneumatic governor of injection pump for leaks (engine 615,616)
- 07-130 - Adjusting governor spring of injection pump (engine 615,616)
- 07-135 - Checking injection nozzles
- 07-137 - Disassembly, cleaning, assembly and adjustment of injection nozzles
- 07-140 - Venting of injection system
- 07-145 - Checking fuel pump and overflow valve
- 07-150 - Checking key starter for leaks

> Assembly jobs

- 07-200 - Removal and installation of injection pump
- 07-205 - Displacing injection pump (after adjusting begin of delivery)
- 07-210 - Replacing pipe connection, pressure valve or copper sealing ring of injection pump
- 07-215 - Replacing diaphragm of injection pump, adjusting compensating path (615,616 M-injection pump w/ pneumatic governor)
- 07-220 - Replacing vacuum box on injection pump
- 07-225 - Replacing altitude adjusting box
- 07-230 - Removal and installation of injection nozzles (injectors)
- 07-235 - Removal and installation of fuel pump
- 07-240 - Removal and installation of injection timer
- 07-245 - Replacing fuel filter

###

Copyright © 2003, 2004 Steve Nervig.
All Rights Reserved