##

## 33 Front Axle

- Bad Wheel Bearing?

> Maintenance Jobs - 1986 through 1993

- 3310 - Front axle, checking, correcting oil level
- 3353 - Checking front axle ball joints
- 3355 - Checking ball joints using special tool

> Maintenance Jobs - 1994 through 1995

- 3353 - Checking front axle ball joints
- 3355 - Checking ball joints using special tool

> Technical data

- 33-0010 - Technical data

> Front axle halves

- 33-0200 - Removing and installing front axle halves
- 33-0260 - Removing and installing front axle shafts (4MATIC)

> Front wheel hub

- 33-0300 - Adjusting wheel bearing play
- 33-0310 - Removing and installing front wheel hub
- 33-0320 - Replacing front wheel hub

> Steering knuckle

- 33-0400 - Removing and installing steering knuckle
- 33-0420 - Removing and installing steering knuckle arm
- 33-0425 - Checking supporting joint of steering knuckle mounting
- 33-0430 - Replacing boot for supporting joint of steering knuckle mounting
- 33-0440 - Replacing supporting joint

> Control arm

- 33-0510 - Removing and installing control arm
- 33-0526 - Replacing control arm mounting

  Misc

- 33-0660 - Replacing rubber bellows on front axle shaft (4MATIC)

- Programmed repairs - Front Axle
  - Select complaint...
- Technical modifications - Front axle

###

Copyright © 2003, 2004, 2005, 2006 Steve Nervig.
All Rights Reserved