##

## 35 Rear Axle

- Bad Wheel Bearing?
- Trailing Arm Bushing Replacement

> Maintenance Jobs - 1986 through 1993

- 3501 - Rear axle oil change
- 3510 - Rear axle, checking, correcting oil level
- 3565 - Rear axle mount, adjusting limiting stop

> Maintenance Jobs - 1994 through 1995

- 3211 - Level control, ADS, ASD fluid level
- 3353 - Checking front axle ball joints
- 3355 - Checking ball joints using special tool
- 3501 - Rear axle oil change

> Rear axle

- 35-010 - Removing and installation of rear axle complete
- 35-040 - Removal and installation of front and rear rubber mounts of rear suspension (See TechMods)
- 35-050 - Removal and installation of rear rubber mounts for center assembly mounting in rear axle bracket (See TechMods)

> Wheel location system

- 35-110 - Removing and installation of camber strut (See TechMods)
- 35-111 - Removing and installation of torque strut (See TechMods)
- 35-112 - Removing and installation of tie rod, replacement of rubber mount (See TechMods)
- 35-113 - Removing and installation of thrust arm (See TechMods)
- 35-114 - Removing and installation of spring link, replacement of rubber mount (See TechMods)
- 35-115 - Removing and installation of wheel carrier
- 35-116 - Replacement of supporting joint on wheel carrier (wheel carrier installed)
- 35-130 - Removal and installation of rear axle shaft flange with angular ball bearing

> Rear axle center assembly

- 35-520 - Removal and installation of rear axle center assembly (See TechMods)
  - - Select model...
- 35-530 - Replacement of radial sealing ring on bevel drive pinion (rear axle center assembly installed)
- 35-540 - Replacement of radial sealing ring on connecting flange of rear axle shaft
  - - Select size...
- 35-620 - Removal and installation of rear axle shafts (See TechMods)
- 35-660 - Replacement of rubber cup seal on rear axle shaft (See TechMods)
- 35-670 - Removal and installation of connecting flange of rear axle shaft

> > - with 185 mm dia ring gear

- M18 - Contents
- 35-0550C - A1 Dismantling and assembling rear axle center assembly, adjusting gear assembly (185 mm dia)
- 35-0560A - M2 Disassembling and assembling differential
- 35-519 - Bleeding the ASD hydraulic system
- 35-519C - K3 Bleeding the ASD hydraulic system (Model W129, W202)
- 35-0545C - F4 Repairing ASD ring cylinder (185 mm dia)
- 35-0560C - E4 Dismantling and assembling ASD differential
- D8 - Testing and repair work
  - D8 thru M9 ...
  - N9 thru C11 ...
  - E11 thru P13...
  - A14 thru K15...
- N15 - Function descriptions, model/equipment combinations
- N16 - Special tools ??
- A17 - Technical modifications
  - - Select mod...
- G18 - Shop made tools
  - - Select tool...
- L18 - Modification note

> > - with 210 mm dia ring gear

- M18 - Contents
- 35-0550D - A1 Dismantling and assembling rear axle center assembly, adjusting gear assembly (210 mm dia)
- 35-0560A - M2 Disassembling and assembling differential
- 35-519 - Bleeding the ASD hydraulic system
- 35-519A - G3 Bleeding the ASD hydraulic system (W140)
- 35-519C - K3 Bleeding the ASD hydraulic system (Model W129, W202)
- 35-0545D - N3 Repairing ASD ring cylinder (210 mm dia)
- 35-0560C - E4 Dismantling and assembling ASD differential
- M10 - Testing and repair work
  - M10 thru O13 ...
  - P13 thru J13 ...
  - P15 thru N16 ...
- A17 - Features, installation survey for rear axle center assemblies (210 mm dia)
- H17 - Technical modifications
  - - Select mod...
- G18 - Shop made tools
  - - Select tool...
- L18 - Modification note

- Technical modifications - Rear axle - wheel location system and drive
- Program Repairs
  - Complaint/type of modification...

###

Copyright © 2003-2006 Steve Nervig.
All Rights Reserved