##

88 Body Panels and Bumpers

- 88-100 - Removal and installation of front fender
- 88-200 - Removal and installation of front bumper
- 88-205 - Removal and installation of molding on front bumper
- 88-210 - Disassembly and assembly of front and rear bumpers
- 88-220 - Removal and installation of rear bumper
- 88-225 - Removal and installation of of molding on rear bumper
- 88-300 - Removal and installation of engine hood
- 88-302 - Adjustment of engine hood
- 88-306 - Removal and installation of engine hood hinge
- 88-310 - Removal and installation of control cable for engine hood
- 88-400 - Removal and installation of radiator cowling
- 88-401 - Removal and installation of radiator grille
- 88-402 - Removal and installation of trim strips on radiator grille
- 88-405 - Removal and installation of Mercedes star
- 88-500 - Removal and installation of trunk lid
- 88-505 - Attachment of model designation on trunk lid
- 88-512 - Removal and installation of hinge lever on trunk lid and soft top compartment cover
- 88-520 - Adjustment of trunk lid
- 88-600 - Removal, installation and adjustment of soft top compartment
- 88-800 - Removal and installation of trim on side wall
- 88-802 - Removal and installation of protective strip on side wall
- 88-830 - Removal and installation of trim on frame side member (coupe)
- 88-855 - Removal and installation of water deflector on front wall pillar and on roof
- 88-860 - Removal and installation of sectional sealing strip on roof frame (coupe)
- 88-900 - Removal and installation of outside mirror
- 88-905 - Removal and installation of electrically adjustable outside mirror

###

©Copyright 2003 Steve Nervig
All Rights Reserved