##

## 30 Acceleration Control System - OM606

- Troubleshooting your Cruise Control
- 30-1010 - Adjusting accelerator control
- 30-1321 - Removing and installing accelerator pedal
- 30-3022 - Removing and installing firewall pivot bearing with accelerator pedal lever
- 30-3402 - Removing and installing, replacing Bowden cable
- 30-4105 - Removing and installing tension-compression damper
- 30-500 - Functional description (for manual transmission version valid up to May 93)
- 30-502 - Hints for troubleshooting
- 30-504 - Testing with adapter
- 30-506 - Testing reference resistor
- 30-541 - Removing and installation of cruise control actuator
- 30-545 - Removing and installation of pushbutton switch
- 30-550 - Removing and installation of sensor (Models 124, 201)
- 30-561 - Adjusting connecting rod or control cable
- 30-565 - Removing and installation of cruise control amplifier
- 30-566 - Removing and installation of cruise control reference resistor
- 30-575 - Removing and installation of switch on clutch pedal (up to May 93)
- 30-576 - Installation of relay against partial load shaking
- 30-577 - Installation of relay against deceleration shaking
- 30-579 - Layout of connectors
- 30-580 - Wiring diagrams

###

©Copyright 2003 Steve Nervig
All Rights Reserved