##

32 Suspension

- George Murphy on installing shocks
- 32-0100 - Removing and installing shock absorber struts
- 32-0110 - Removing and installing rear shock absorber
- 32-0120 - Checking shock absorber strut (front)
- 32-0121 - Testing shock absorbers (rear)
- 32-0200 - Removing and installing front springs
- 32-0230 - Removing and installing rear springs
- 32-0250 - Test value for springs
- 32-0300 - Removing and installing front torsion bar
- 32-0310 - Removing and installing rear torsion bar
- 32-0501 - Function description
- 32-0510 - Testing rear axle spring struts
- 32-0515 - Testing front axle spring struts for leaks (Model 201)
- 32-0520 - Testing spring actuators on front and rear axles
- 32-0530 - Removing pressure oil pump and level controller on rear axle (w/ level control)
- 32-0537 - Testing pressure oil pump, distributor valve and level controller (Model 201)
- 32-0540 - General function test (Model 201)
- 32-0550 - Testing distributor valve for internal leaks (Model 201)
- 32-0570 - Testing function of electrical control valve (Model 201)
- 32-0580 - Testing function of electrical check valve (Model 201)
- 32-0610 - Removing and installing rear axle spring struts
- 32-0615 - Removing and installing front axle spring struts (Model 201)
- 32-0620 - Removing and installing spring actuators (Model 201)
- 32-0630 - Emptying and filling pressure oil system
- 32-0640 - Remove and installing pressure oil pump
- 32-0645 - Replacing radial sealing ring of pressure oil pump (Engine M102,601,602,603)
- 32-0660 - Removing and installing control rod/connecting rod on level controller
- 32-0670 - Removing and installing level controller
- 32-0680 - Removing and installing distributor valve (Model 201)
- 32-0690 - Removing and installing electrical control valve (Model 201)
- 32-0700 - Removing and installing electrical check valve (Model 201)
- Programmed repairs - Level control
  - Select complaint...

###

©Copyright 2003 Steve Nervig
All Rights Reserved