##

## 14 Intake Manifold, Exhaust Manifold, Emissions Control System - M103

> Maintenance Jobs - 1986 through 1993

- 1480 - Replacing oxygen sensor

> Service Information

- Service Intro - Model Year 1992, Model 124 (USA), Introduction into Service

> Emissions control

- 14-0001 - Distinguishing features of vehicles with emissions control system
- 14-0115 - Testing catalytic converter warning system (J) - (Tech Mods)
- 14-0116 - Testing oxygen sensor failure indicator (USA) - (See also Group 07)
- 14-0490 - Converting USA tourist vehicles with catalytic converter

> Intake manifold

- 14-1310 - Removing and installing intake manifold, replacing gasket - (Tech Mods)
- 14-1346 - Replacing intake manifold (intake manifold removed)

> Exhaust manifold

- 14-3915 - Removing and installing exhaust manifold - (Tech Mods) - (Tech Mods)

> Air pump

- 14-7165 - Testing air pump
- 14-7251 - Removing and installing air pump - (Tech Mods)
- 14-7252 - Removing and installing electromagnetic clutch
- 14-7253 - Removing and installing air injection/transmission shiftpoint retard relay
- 14-7305 - Removing and installing air pump switchover valve

> EGR

- 14-7611 - Testing exhaust gas recirculation - (Tech Mods)
- 14-7692 - Removing and installing exhaust gas recirculation switchover valve (only (J) (USA))

###

Copyright © 2003-2008 Steve Nervig.
All Rights Reserved