##

## 46 Steering System

> Maintenance Jobs - 1986 through 1993

- 4611 - Checking power steering fluid level
- 4650 - Checking steering play
- 4671 - Retightening steering bolts

> Maintenance Jobs - 1994 through 1995

- 4611 - Checking power steering fluid level
- 4650 - Checking steering play
- 4671 - Retightening steering bolts

> Service Information

- Service Intro - Model Year 1992, Model 124 (USA), Introduction into Service
- Service Intro - Model Year 1992, Model 124 Sportline (USA), Introduction into Service
- Service Intro - Model Year 1992, 400E/500E, Introduction into Service

> Survey steering

- 46-0001 - Survey of steering gears
- 46-0002 - Survey of power steering pumps (LHP)/tandem pumps (TANP)
- 46-0003 - Survey of steering linkage

> Checking steering gear

- 46-0110 - Checking play of steering components
- 46-0120 - Checking and adjusting friction torque of steering gear
- 46-0140 - Replacing steering gear when performing repairs to vehicle involved in accident
- 46-3070 - Testing oil pressure of power steering pump

> Repairing steering gear

- 46-0230 - Important notes regarding repair of steering gear
- 46-0231 - Removing and installing parameter steering (PML) P-valve (Y10)
- 46-0232 - Removing, installing and checking bearing cover with pitman arm shaft
- 46-0233 - Disassembling and assembling pitman arm shaft/bearing cover
- 46-0234 - Removing and installing adjusting screw
- 46-0235 - Removing, installing and checking play compensator
- 46-0236 - Removing and installing steering/bearing cover, replacing radial seal ring
- 46-0238 - Removing, installing and checking control valve

> Repairing power steering pump

- 46-0715 - Filling and bleeding the power steering pump/tandem pump
- 46-0730 - Disassembling and assembling power steering pump/tandem pump

> Steering gear and pitman arm

- 46-3230 - Adjusting steering gear in vehicle
- 46-3265 - Removing, installing, replacing sealing ring in lower housing cover
- 46-3400 - Removing and installing of steering gear

> Power steering pump

- 46-4000 - Removing and installing power steering pump
- 46-4080 - Filling and bleeding power steering pump

> Steering linkage and idler arm

- 46-6177 - Removing and installing drag link
- 46-6317 - Removing and installing steering idler arm, replacing plain rubber mount
- 46-7007 - Removing and installing tie rod
- 46-7202 - Replacing boot for tie rod ball joint and drag link ball joint

> Wheel, jacket tube, shaft, lock

- 46-7700 - Removing, checking and installing jacket tube
- 46-7740 - Dismantling and assembling jacket tube
- 46-8010 - Removing and installing the steering lock complete
- 46-8110 - Removing and installing lock cylinder
- 46-8240 - Removing and installing steering wheel
- 46-8300 - Removing and installing contact spiral
- 46-8310 - Removing and installing steering angle sensor
- 46-8340 - Removing and installing slip ring on steering wheel
- Programmed repairs - Steering
  - Select complaint...
- Programmed repairs - Steering gear and power steering pumps
  - Select complaint...
- Technical modifications - Steering
- Technical modifications - Steering gear 765.9 and power steering pumps

###

Copyright © 2003-2008 Steve Nervig.
All Rights Reserved