##

## 14 Intake Manifold, Exhaust Manifold, Emissions Control System - M104

> Maintenance Job - 1990 through 1993

- 1480 - Replacing oxygen sensor

> Service Information

- Service Intro - Model Year 1992, Model 124 (USA), Introduction into Service

> General

- 14-0010 - Intake manifold
- 14-0020 - Exhaust manifold

> Emissions control

- 14-0030 - Emissions control system (vacuum diagram)

> Intake manifold

- 14-1310 - Removing and installing intake manifold, replacing gasket - (See also Group 09)
- 14-1346 - Replacing intake manifold (intake manifold removed)

> Exhaust manifold

- 14-3915 - Removing and installing exhaust manifold
- 14-3915G - Removing and installing exhaust manifold (M104.94/99)

> Lambda sensor

- 14-5303D - Removing and installing lambda sensor (M104.94/99)

> Air pump

- 14-7251 - Removing and installing air pump
- 14-7251D - Removing and installing air pump
- 14-7252D - Removing and installing air pump belt pulley
- 14-7264 - Removing and installing electromagnetic clutch
- 14-7264D - Removing and installing electromagnetic coupling
- 14-7305 - Removing and installing air pump switchover valve

> EGR

- 14-7662 - Removing and installing exhaust gas recirculation valve
- 14-7692 - Removing and installing exhaust gas recirculation switchover valve (only (J) (USA))

###

Copyright © 2003-2008 Steve Nervig.
All Rights Reserved