##

## 18 Lubrication System - M104

> General

- 18-0020 - Engine oil and filter change
- 18-0050 - Oil circuit
- 18-0070 - Testing oil pressure
- 18-0090 - Operation of oil pressure gauge
- 18-0250 - Measuring oil consumption

> Oil filter

- 18-1000 - Operation of oil filter
- 18-1100 - Removing and installing oil filter
- 18-1120 - Removing and installing oil pipes (oil filter - air-to-oil cooler)

> Oil cooler

- 18-1300 - Removing and installing air-to-oil cooler
- 18-1320 - Removing and installing oil-to-coolant heat exchanger
- 18-1370 - Pressure-testing oil-to-coolant heat exchanger

> Oil pump

- 18-2100 - Removing and installing oil pump
- 18-2120 - Replacing and riveting oil pump chain
- 18-2150 - Removing and installing oil pressure relief valve in oil pump
- 18-2180 - Removing and installing oil shield at crankshaft

> Oil gauge, sensor, transport

- 18-3100 - Function of electrical oil level indicator
- 18-3300 - Removing and installing oil level sensor
- 18-3320 - Testing oil level sensor
- 18-3500 - Checking dipstick and guide tube
- 18-3510 - Removing and installing dipstick guide tube, W202
- 18-4000 - Removing and installing oil spray nozzles for pistons
- 18-4100 - Removing and installing oil spray nozzles for timing chain, M104.94/99
- 18-4150 - Replacing oil non-return valve of chain tensioner

###

Copyright © 2003-2008 Steve Nervig.
All Rights Reserved