##

## 03 Crank Assembly - M103

> Crankshaft

- 03-1800 - Removing and installing crankshaft

> Connecting rods

- 03-3100 - Checking, replacing and tightening conrod bolts
- 03-3130 - Servicing, aligning and mounting conrod in bearings

> Pistons

- 03-3160 - Removing and installing pistons
- 03-3165 - Pistons, matching and dimensions
- 03-3170 - Replacing piston rings

> Assembly

- 03-3180 - Checking and servicing crankshaft
- 03-3200 - Mounting crankshaft in bearings
- 03-3240 - Replacing front crankshaft radial seal
- 03-3270 - Replacing rear crankshaft radial seal
- 03-3300 - Removing and installing grooved ball bearing and end cover in crankshaft
- 03-3420 - Removing and installing belt pull/vibration damper and hub
- 03-3450 - Checking, correcting setting of TDC sensor

> Flywheel

- 03-4100 - Removing and installing flywheel or driven plate
- 03-4200 - Machining flywheel (except two-mass flywheel)
- 03-4300 - Replacing ring gear
- 03-4600 - Function of two-mass flywheel
- 03-4620 - Removing and installing two=mass flywheel
- 03-4640 - Removing and installing needle bush in two-mass flywheel
- 03-5000 - Removing and installing holding lock for crankshaft/ring gear

###

Copyright © 2003-2008 Steve Nervig.
All Rights Reserved