##

07.1 Injection System - OM617 turbo

> Survey and operation

- 07.1-001 - Survey model - engine - injection pump
- 07.1-010 - Operation injection pump with governor
- 07.1-015 - Operation engine-transmission-overload protection

> Testing and adjusting jobs

- 07.1-100 - Adjustment of idle speed and idle speed adjuster
- 07.1-105 - Checking maximum speed at no load
- 07.1-108 - Checking injection timing (begin of delivery) with digital tester (RIV method)
- 07.1-109 - Checking injection timing (begin of delivery) (high pressure method)
- 07.1-110 - Checking injection timing (begin of delivery) (flow pressure method)
- 07.1-111 - Checking injection timing (begin of delivery) (position indicator RIV method)
- 07.1-114 - Checking injection timing (begin of delivery) with digital tester (RIV method) - following checkup
- 07.1-115 - Checking injection timing (begin of delivery) (high pressure method) - following checkup
- 07.1-116 - Checking injection timing (begin of delivery) (position indicator RIV method) - following checkup
- 07.1-135 - Checking injection nozzles
- 07.1-137 - Disassembly, cleaning, assembly and adjustment of injection nozzles
- 07.1-140 - Venting Injection System
- 07.1-145 - Checking fuel pump and bypass valve
- 07.1-150 - Checking vacuum shutoff for leaks

> Assembly jobs

- 07.1-200 - Removal and installation of injection pump
- 07.1-201 - Installation of injection pump (with locking screw)
- 07.1-210 - Replacement of pipe connection, delivery valve or copper sealing ring on injection pump
- 07.1-220 - Replacement of vacuum control unit at injection pump
- 07.1-230 - Removal and installation of injection nozzles
- 07.1-235 - Removal and installation of fuel pump
- 07.1-240 - Removal and installation of injection timing device

###

Copyright © 2003, 2004 Steve Nervig.
All Rights Reserved.