##

20 Cooling System - M110

> Cooling system

- 20-005 - Coolant circuit and engine cooling
- 20-010 - Draining and filling coolant Anti-freeze table
- 20-015 - Cleaning cooling system

> Coolant pump

- 20-210 - Removal and installation of water pump

> Viscofan clutch, temperature controlled

- 20-310 - Temperature controlled visco-fan clutch
- 20-330 - Magnetic fan clutch

> Radiator

- 20-420 - Removal and installation of radiator
- 20-425 - Repairing radiator
- 20-430 - Testing radiator or expansion tank closing cap

> More information

- Oil in cooling system? Use Alkaline cleaner, disodiumtrixosilicate-pentahydrate.
  - Part number is 001 986 21 71 (500 grams)
- Scale in cooling system? Use Citric Acid at 100 grams per liter.
  - Part number is 000 989 10 25 (500 grams)
- Cooling System Diagnostic

###

Copyright © 2003, 2004 Steve Nervig.
All Rights Reserved