##

03 Engine, Internals - OM606

- 03-1101HA - Checking, correcting setting of bracket of TDC sensor
  - G14 - Check, correct position of bracket of TDC Sensor
- 03-1600HA - Removing, installing belt pulley/ vibration damper
  - L16 - Remove the pulley / vibration damper
- 03-1600HB - Belt pulley/vibration damper as-built configuration
- 03-1600HC - Belt pulley/vibration damper as-built configuration
- 03-1600HD - Belt pulley/vibration damper as-built configuration
- 03-1600HE - Belt pulley/vibration damper as-built configuration
- 03-3000HA - Replacing front crankshaft radial seal
  - E15 - Installing front crankshaft radial seal
- 03-3063HA - Replacing rear crankshaft radial seal
  - H15 - Installing rear crankshaft radial seal
- 03-4351B - Removing and installing crankshaft
  - K15 - Examining bolts of crankshaft bearing caps
- 03-4355A - Measuring crankshaft and installing bearings
  - M15 - Installing crankshaft radially in bearings
  - C16 - Assigning crankshaft bearing shells
  - G16 - Installing crankshaft axially in bearings
- 03-5000HA - Installing, removing retaining lock for crankshaft/starter ring gear
- 03-6111HA - Testing, repairing connecting rod
  - K14 - Tightening connecting rod bolts
  - L14 - Press-fitting new connecting rod bush
  - N14 - Aligning connecting rod
  - A15 - Checking connecting rod bolts
- 03-7021B - Removing, and installing pistons
  - B15 - Removing, installing oil deflector plate
  - C15 - Measuring piston projection
- 03-7311HA - Removing and installing pistons rings
- 03-8001HA - Removing and installing flywheel/driven plate
  - M16 - Examining bolts for flywheel / driven plate
- 03-8022A - Checking, remachining flywheel
- 03-8312A - Replacing ring gear of flywheel
- 03-8400A - Removing, installing needle bush in two-mass flywheel
- 03-8400HA - Removing, installing grooved ball bearing of crankshaft

###

©Copyright 2003 Steve Nervig
All Rights Reserved