##

## 30 Acceleration Control System - M103

> Maintenance Jobs - 1986 through 1993

- 3022 - Inspecting, lubricating throttle linkage

  Additional Information

- Troubleshooting your Cruise Control
- ASD, ASR, 4MATIC - Driving Dynamic Systems: ASD, ASR and 4MATIC

> Accelerator control

- 30-0010 - Lubricating accelerator control linkage, checking ease of movement and wear (after engine wash)
- 30-0310 - Removing and installing engine longitudinal accelerator control shaft
- 30-0320 - Removing, installing and adjusting chassis accelerator control shaft, Model 107
- 30-0355 - Notes for test and repair work on vehicles with ASR (See also Group 42)
- 30-0360 - ABS/ASR and electronic accelerator pedal initial test
- 30-1010 - Adjusting accelerator control - (Tech Mods)
- 30-1050 - Testing electronic engine control
- 30-1151 - Removing and installing electronic accelerator pedal control unit
- 30-1152 - Removing and installing electronic accelerator pedal actuator
- 30-1156 - Removing and installing electronic accelerator pedal position sensor - (Tech Mods)
- 30-1321 - Removing and installing accelerator pedal
- 30-3022 - Removing and installing fire wall bearing with accelerator pedal lever
- 30-3402 - Removing, installing and adjusting Bowden cable - (Tech Mods)

> Cruise control / Tempomat

- 30-500 - Functional description (for manual transmission version valid up to May 93)
- 30-502 - Hints for troubleshooting
  - Select complaint...
- 30-504 - Testing with adapter
- 30-506 - Testing reference resistor
- 30-541 - Removing and installation of cruise control actuator
- 30-545 - Removing and installation of pushbutton switch
- 30-550 - Removing and installation of sensor (Models 124, 201)
- 30-561 - Adjusting connecting rod or control cable
- 30-565 - Removing and installation of cruise control amplifier
- 30-566 - Removing and installation of cruise control reference resistor
- 30-575 - Removing and installation of switch on clutch pedal (up to May 93)
- 30-576 - Installation of relay against partial load shaking
- 30-577 - Installation of relay against deceleration shaking
- 30-579 - Layout of connectors
- 30-580 - Wiring diagrams
- 30-7300 - Testing Tempomat cruise control, vehicles with ASR
- Modification Notes
- Programmed Repair - Tempomat / cruise control
- Technical Revisions - Cruise control / Tempomat - Models 124, 129, 140, 201

###

Copyright © 2003-2012 Steve Nervig.
All Rights Reserved