## 00 Maintenance Jobs - 1981 through 1993

- Introduction - Maintenance Manual Model Year 1981 to 1993
  - - - Select page...
  - 0050 - Inspecting component condition
  - 0051 - Inspecting condition of lines and hoses
  - 0053 - Inspecting components, lines and hoses
  - 0090 - Suspension and body structure inspection
  - 0091 - Water leakage and corrosion inspection
  - 0101 - Engine oil and filter change
  - 0560 - Adjusting valve clearance - M110, OM616, OM617
  - 0561 - Checking valve clearance - M102.983
  - 0750 - Checking and adjusting idle speed - OM601
  - 0758 - Checking and adjusting idle speed - M110
  - 0760 - Checking injection timing - (diesel)
  - 0761 - Adjusting injection timing - (diesel)
  - 0780 - Replacing fuel filter
  - 0781 - Replacing fuel prefilter - (diesel)
  - 0932 - Cleaning metal-reinforced air filter element - (diesel)
  - 0980 - Replacing air filter element
  - 0981 - Replacing air filter elements - M116, M117
  - 1350 - Checking condition and tension of V-belts
  - 1351 - Inspecting poly-V-belt
  - 1470 - Checking intake/exhaust manifold seating - OM616, OM617
  - 1480 - Replacing oxygen sensor
  - 1550 - Check spark plugs, replace if necessary
  - 1580 - Replacing spark plugs
  - 2010 - Checking coolant level/antifreeze protection
  - 2011 - Checking coolant level
  - 2050 - Checking cooling and heating system
  - 2080 - Replacing coolant
  - 2290 - Adjust engine stop, retorque engine mount bolts - OM616, OM617
  - 2291 - Adjust engine stop - OM616, OM617
  - 2551 - Checking clutch disk for wear
  - 2601 - Manual transmission oil change
  - 2610 - Manual transmission, checking, correcting oil level
  - 2702 - Automatic transmission fluid and filter change
  - 2710 - Automatic transmission, checking, correcting fluid level
  - 2801 - Transfer case fluid change
  - 2810 - Transfer case, checking, correcting fluid level
  - 2910 - Clutch system, checking, correcting fluid level
  - 2950 - Clutch system, inspect
  - 3022 - Inspecting, lubricating throttle linkage
  - 3052 - Checking and adjusting idle speed adjuster - OM616, OM617
  - 3211 - Level control, ADS, ASD, 4MATIC, fluid level
  - 3251 - Inspecting self-leveling suspension
  - 3310 - Front axle, checking, correcting oil level
  - 3353 - Checking front axle ball joints
  - 3355 - Checking ball joints using special tool
  - 3501 - Rear axle oil change
  - 3510 - Rear axle, checking, correcting oil level
  - 3565 - Rear axle mount, adjusting limiting stop
  - 4050 - Inspecting/rotating wheels
  - 4051 - Checking tires
  - 4060 - Correcting tire pressure
  - 4070 - Tightening wheel bolts
  - 4152 - Inspecting drive shaft flexible coupling
  - 4210 - Checking brake fluid level
  - 4250 - Inspecting brake lines for damage
  - 4251 - Checking brake pad/disk thickness
  - 4252 - Inspecting, cleaning brake disks
  - 4256 - Inspecting parking brake cable
  - 4261 - Adjusting parking brake
  - 4280 - Replacing brake fluid
  - 4290 - Brake test, parking brake check
  - 4611 - Checking power steering fluid level
  - 4650 - Checking steering play
  - 4671 - Retightening steering bolts
  - 4750 - Checking fuel system condition
  - 4970 - Retightening exhaust flange
  - 4971 - Retightening exhaust system connections
  - 5410 - Checking and correcting battery fluid level
  - 5451 - Checking warning and indicator lamps
  - 6030 - Cleaning water drains
  - 6190 - Removing and installing engine compartment lower panel
  - 7220 - Lubricating door hinges
  - 7221 - Lubricating door locks
  - 7710 - Hydraulic top, checking and correcting fluid level
  - 7730 - Sun roof, clean and grease rails
  - 7750 - Soft top, checking locking tabs
  - 8210 - Checking, correcting windshield washer fluid level
  - 8230 - Cleaning cassette deck tone head
  - 8231 - Cleaning antenna mast
  - 8251 - Headlamp and exterior lamp inspection
  - 8252 - Windshield and headlamp wiper/washer inspection
  - 8280 - Replacing windshield wiper blade
  - 8312 - Checking, correcting A/C refrigerant charge
  - 8381 - Replacing dust filter for heating/ventilation
  - 8382 - Replacing active charcoal filter
  - 8383 - Replacing recirculating air filter
  - 8820 - Lubricating folding side mirror
  - 8821 - Lubricating hood
  - 9150 - Inspecting safety belts for damage
  - 9151 - Backrest lock - check operation
  - 9490 - Removing and installing lower noise encapsulation panels
  - 9850 - Checking body for paint damage

  Back to 00 Maintenance
  Copyright 2003-2008 Steve Nervig.
  All Rights Reserved